|  |  |  |  |
| --- | --- | --- | --- |
| TEST CASE # | COMPONENT | TEST CASE | RESULT |
|  | RED LED | On when push button is pressed for more than 2 secs. | Pass |
|  | BLUE LED | On when push button is pressed once for less than 2 secs after the red led is on with frequency 1Hz,4Hz,8Hz. | Pass |
|  | GREEN LED | On when push button is pressed once for less than 2 secs after the red led is on with frequency 1Hz,4Hz,8Hz. | Pass |
|  | ORANGE LED | On when push button is pressed once for less than 2 secs after the red led is on with frequency 1Hz,4Hz,8Hz. | Pass |
|  | ALL 3 leds | Off after the push buuton has been pressed once again. | Pass |
|  | RED LED | Off after pushbutton is pressed for more than 2 secs. | Pass |